Vexta C7080-9212K-C2 Special Offer X48

  * Especificaciones Tecnicas :: Datos Clave

    * Marca:

            Vexta

            (Oriental Motor U.S.A. Corp.)

    * Origen:

            Made In Japan

    * Modelo:

            C7080-9212K-C2

    * Brida: 

            NEMA 23

            (56.00mm x 56.00mm) 

    * Cuerpo (Formato): 

            Cuasi-Cúbico 

    * Cuerpo (Dimensiones): 

            60.00mm x 56.00mm x 56.00mm

            (Alto x Largo x Ancho) 

    * Eje (Diámetro): 

            6.35mm 

    * Eje (Longitud): 

            19.05mm 

    * Torque De Mantenimiento (Máximo): 

            1.150 Newtons.Metro

            115.0 Newtons.Centímetro

            10.25 Kilogramos.Centímetro

            (Bipolar-Serie) 

            1.150 Newtons.Metro

            115.0 Newtons.Centímetro

            10.25 Kilogramos.Centímetro

            (Bipolar-Paralelo)  

            0.82 Newtons.Metro

            82.00 Newtons.Centímetro

            7.250 Kilogramos.Centímetro

            (Unipolar)  

    * Exactitud: 

            1.8º / Paso

            (200 Pasos Por Vuelta) 

    * Peso: 

            0.55 Kilogramos 

    * Corriente: 

            0.71 Amperios Por Fase

            (Modalidad Corriente Constante)

            (Bipolar-Serie)

            1.42 Amperios Por Fase

            (Modalidad Corriente Constante)

            (Bipolar-Paralelo)  

            1.01 Amperios Por Fase

            (Modalidad Corriente Constante)

            (Unipolar) 

    * Tensión: 

            8.00 Voltios Por Fase

            (Modalidad Tensión Constante)

            (Bipolar-Serie)  

            4.00 Voltios Por Fase

            (Modalidad Tensión Constante)

            (Bipolar-Paralelo)  

            5.66 Voltios Por Fase

            (Modalidad Tensión Constante) 

            (Unipolar)  

    * Resistencia: 

            12.40 Ohmios Por Fase

            (Bipolar-Serie) 

            3.10 Ohmios Por Fase

            (Bipolar-Paralelo)

            6.20 Ohmios Por Fase  

            (Unipolar) 

    * Número De Cables: 

            4

            (Bipolar-Serie)

            6

            (Bipolar-Serie / Unipolar)

            8

            (Universalmente Configurables)

    * Conexionado Interno: 

            Bipolar-Serie

            Bipolar-Serie / Unipolar

            Flotante

            (Universalmente Configurable Desde El Exterior)

    * Conexionado Externo: 

            Bipolar-Serie

            (2 Fases) 

            Bipolar-Paralelo

            (2 Fases)

            Unipolar

            (4 Fases)  

    * Especificaciones Tecnicas :: Hoja De Datos

    * Motor Type:

            2-Phase

    * Motor Frame Size:

             2.22 in. sq.

            (56 mm. sq.) 

    * Gear/ Shaft Type:

            Round Shaft

    * Connection Type:

            Bipolar (Series)

    * Lead Wires:

            4

    * Current Per Phase (A/Phase):

            0.71 A/Phase

            Bipolar (Series)

    * Encoder:

            Not Equipped

    * Shaft:

            Single

    * Step Angle:

            1.8°

    * Maximum Holding Torque (lb-in):

            9.2 lb-in

            [Bipolar (Series)]

    * Rotor Inertia (oz-in2):

            0.66 oz-in2

    * RoHS Compliant:

            Yes

    * Available to Ship:

            Same Day

            (If Ordered By 12pm PST)

            (1-10 Pcs)

    * Insulation Resistance:

            100 M minimum under normal temperature and humidity, when measured by a 500 VDC megger between the motor coils and casing.

    * Dielectric Strength:

            Sufficient to withstand 1.0 kV, 60 Hz applied between the motor coils and casing for 1 minute, under normal temperature and humidity.

    * Temperature Rise:

            Temperature rise of the coil measured by the Change Resistance Method is 144°F (80°C) or less (at standstill, two phases energized).

    * Insulation Class:

            Class B

            [266°F (130°C)]

    * Ambient Temperature Range:

            14°F ~ 122°F

            (-10°C ~ 50°C)

    * Ambient Humidity:

            85% Or Less

    * Shaft Runout:

            0.002 in (0.05 mm) T.I.R. at top of output shaft

    * Concentricity:

            0.003 in. (0.075 mm) T.I.R.

    * Perpendicularity:

            0.003 in. (0.075 mm) T.I.R.

    * Radial Play:

            0.001 inch (0.025 mm) max. of 1.12 lb. (5 N)

    * Axial Play:

            0.003 in (0.075 mm) max. of 2.2 lb. (10 N)

    * Step Accuracy:

            ±3 arc minutes (±0.05°)

