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  0 to 30V,0 to 5A
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  Ideal DC Source for Lab,Service,Industry and Education
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  Excellent Stability and Precise Voltage & Current Level
   Setting
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  Adjustable Constant Voltage/Current & Overload Indication
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  Isolated Outputs for Series or Parallel Operation
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  3 Digit LED Read-outs
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  Low Noise and Ripple
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  Superior Line/Load Regulation


	


	Protek DF1730SL10A
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 0-30V 0-10 A
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 DOBLE display digital. 
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 Regulación fina de tensión y corriente 


